commit 643f6acc4bb2d799bebd54c973949c1a90eb26a3
Author: Eric Sandeen <sandeen@redhat.com>
Date:   Tue Jun 21 12:55:15 2016 +1000

    xfs_repair: set rsumino version to 2

    If we run xfs/033 with "-m crc=0", the test fails with a repair
    output difference:

         Phase 7 - verify and correct link counts...
        +resetting inode INO nlinks from 0 to 1
         done

    This is because when we zero out the realtime summary inode and
    rebuild it, we set its version to 1, then set its ip->i_d.di_nlink
    to 1.  This is a little odd, because v1 inodes store their link
    count in di_onlink...

    Then, later in repair we call xfs_inode_from_disk(), which sees the
    version one inode, and converts it to version 2 in part by copying
    di_onlink to di_nlink.  But we never *set* di_onlink, so di_nlink
    gets reset to zero, and this error is discovered later in repair.

    Interestingly, mk_rbmino() was changed in 138659f1 to set version 2;
    it looks like mk_rsumino was just missed.

    Signed-off-by: Eric Sandeen <sandeen@redhat.com>
    Reviewed-by: Dave Chinner <dchinner@redhat.com>
    Signed-off-by: Dave Chinner <david@fromorbit.com>

Index: xfsprogs-4.5.0/repair/phase6.c
===================================================================
--- xfsprogs-4.5.0.orig/repair/phase6.c
+++ xfsprogs-4.5.0/repair/phase6.c
@@ -507,7 +507,7 @@ mk_rbmino(xfs_mount_t *mp)
			error);
	}

-	vers = xfs_sb_version_hascrc(&mp->m_sb) ? 3 : 1;
+	vers = xfs_sb_version_hascrc(&mp->m_sb) ? 3 : 2;
	memset(&ip->i_d, 0, xfs_icdinode_size(vers));

	ip->i_d.di_magic = XFS_DINODE_MAGIC;
@@ -766,7 +766,7 @@ mk_rsumino(xfs_mount_t *mp)
			error);
	}

-	vers = xfs_sb_version_hascrc(&mp->m_sb) ? 3 : 1;
+	vers = xfs_sb_version_hascrc(&mp->m_sb) ? 3 : 2;
	memset(&ip->i_d, 0, xfs_icdinode_size(vers));

	ip->i_d.di_magic = XFS_DINODE_MAGIC;
