From 84b8c9ceaa5257f7ff4ab059ff208246ecdfe9d9 Mon Sep 17 00:00:00 2001
From: Michael Munday <munday@ca.ibm.com>
Date: Tue, 17 Jan 2017 11:33:38 -0500
Subject: [PATCH] syscall: expose IfInfomsg.X__ifi_pad on s390x

Exposing this field on s390x improves compatibility with the other
linux architectures, all of which already expose it.

Fixes #18628 and updates #18632.

Change-Id: I08e8e1eb705f898cd8822f8bee0d61ce11d514b5
---

diff --git a/src/syscall/ztypes_linux_s390x.go b/src/syscall/ztypes_linux_s390x.go
index 63c4a83..b589425 100644
--- a/src/syscall/ztypes_linux_s390x.go
+++ b/src/syscall/ztypes_linux_s390x.go
@@ -449,12 +449,12 @@
 }
 
 type IfInfomsg struct {
-	Family uint8
-	_      uint8
-	Type   uint16
-	Index  int32
-	Flags  uint32
-	Change uint32
+	Family     uint8
+	X__ifi_pad uint8
+	Type       uint16
+	Index      int32
+	Flags      uint32
+	Change     uint32
 }
 
 type IfAddrmsg struct {
