From 7c71188610b4ceba0339c2bc884320bcb749adee Mon Sep 17 00:00:00 2001
From: Anuj Phogat <anuj.phogat@gmail.com>
Date: Wed, 20 Sep 2017 12:11:03 -0700
Subject: [PATCH] intel: Change a KBL pci id to GT2 from GT1.5

See Mesa commit 9c588ff

Cc: Matt Turner <mattst88@gmail.com>
Cc: Rodrigo Vivi <rodrigo.vivi@intel.com>
Signed-off-by: Anuj Phogat <anuj.phogat@gmail.com>
Reviewed-by: Rodrigo Vivi <rodrigo.vivi@intel.com>
Signed-off-by: Rodrigo Vivi <rodrigo.vivi@intel.com>
---
 intel/intel_chipset.h | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/intel/intel_chipset.h b/intel/intel_chipset.h
index 3ff59ad..d81b164 100644
--- a/intel/intel_chipset.h
+++ b/intel/intel_chipset.h
@@ -202,7 +202,7 @@
 #define PCI_CHIP_KABYLAKE_ULX_GT1	0x590E
 #define PCI_CHIP_KABYLAKE_ULX_GT2	0x591E
 #define PCI_CHIP_KABYLAKE_DT_GT2	0x5912
-#define PCI_CHIP_KABYLAKE_DT_GT1_5	0x5917
+#define PCI_CHIP_KABYLAKE_M_GT2		0x5917
 #define PCI_CHIP_KABYLAKE_DT_GT1	0x5902
 #define PCI_CHIP_KABYLAKE_HALO_GT2	0x591B
 #define PCI_CHIP_KABYLAKE_HALO_GT4	0x593B
@@ -434,7 +434,6 @@
 
 #define IS_KBL_GT1(devid)	((devid) == PCI_CHIP_KABYLAKE_ULT_GT1_5	|| \
 				 (devid) == PCI_CHIP_KABYLAKE_ULX_GT1_5	|| \
-				 (devid) == PCI_CHIP_KABYLAKE_DT_GT1_5	|| \
 				 (devid) == PCI_CHIP_KABYLAKE_ULT_GT1	|| \
 				 (devid) == PCI_CHIP_KABYLAKE_ULX_GT1	|| \
 				 (devid) == PCI_CHIP_KABYLAKE_DT_GT1	|| \
@@ -446,6 +445,7 @@
 				 (devid) == PCI_CHIP_KABYLAKE_ULT_GT2F	|| \
 				 (devid) == PCI_CHIP_KABYLAKE_ULX_GT2	|| \
 				 (devid) == PCI_CHIP_KABYLAKE_DT_GT2	|| \
+				 (devid) == PCI_CHIP_KABYLAKE_M_GT2	|| \
 				 (devid) == PCI_CHIP_KABYLAKE_HALO_GT2	|| \
 				 (devid) == PCI_CHIP_KABYLAKE_SRV_GT2	|| \
 				 (devid) == PCI_CHIP_KABYLAKE_WKS_GT2)
-- 
2.9.5

