# -*- cfg-sha: 56176386deef83f9f1fd9d1c143a20be1294c8ed5e720aaef37e4b007ccbbde3
# BSD LICENSE
# Copyright(c) 2010-2014 Intel Corporation. All rights reserved.
# All rights reserved.
# Redistribution and use in source and binary forms, with or without
# modification, are permitted provided that the following conditions
# are met:
# * Redistributions of source code must retain the above copyright
# notice, this list of conditions and the following disclaimer.
# * Redistributions in binary form must reproduce the above copyright
# notice, this list of conditions and the following disclaimer in
# the documentation and/or other materials provided with the
# distribution.
# * Neither the name of Intel Corporation nor the names of its
# contributors may be used to endorse or promote products derived
# from this software without specific prior written permission.
# THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
# "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
# LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
# A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT
# OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
# SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
# LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
# DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY
# THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
# (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
# OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
# BSD LICENSE
# Copyright(c) 2010-2016 Intel Corporation. All rights reserved.
# All rights reserved.
# Redistribution and use in source and binary forms, with or without
# modification, are permitted provided that the following conditions
# are met:
# * Redistributions of source code must retain the above copyright
# notice, this list of conditions and the following disclaimer.
# * Redistributions in binary form must reproduce the above copyright
# notice, this list of conditions and the following disclaimer in
# the documentation and/or other materials provided with the
# distribution.
# * Neither the name of Intel Corporation nor the names of its
# contributors may be used to endorse or promote products derived
# from this software without specific prior written permission.
# THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
# "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
# LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
# A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT
# OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
# SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
# LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
# DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY
# THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
# (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
# OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
# BSD LICENSE
# Copyright(c) 2010-2017 Intel Corporation. All rights reserved.
# All rights reserved.
# Redistribution and use in source and binary forms, with or without
# modification, are permitted provided that the following conditions
# are met:
# * Redistributions of source code must retain the above copyright
# notice, this list of conditions and the following disclaimer.
# * Redistributions in binary form must reproduce the above copyright
# notice, this list of conditions and the following disclaimer in
# the documentation and/or other materials provided with the
# distribution.
# * Neither the name of Intel Corporation nor the names of its
# contributors may be used to endorse or promote products derived
# from this software without specific prior written permission.
# THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
# "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
# LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
# A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT
# OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
# SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
# LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
# DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY
# THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
# (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
# OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
# RTE_EXEC_ENV values are the directories in mk/exec-env/
CONFIG_RTE_EXEC_ENV="linuxapp"
# RTE_ARCH values are architecture we compile for. directories in mk/arch/
CONFIG_RTE_ARCH="x86_64"
# machine can define specific variables or action for a specific board
# RTE_MACHINE values are architecture we compile for. directories in mk/machine/
CONFIG_RTE_MACHINE="default"
# The compiler we use.
# RTE_TOOLCHAIN values are architecture we compile for. directories in mk/toolchain/
CONFIG_RTE_TOOLCHAIN="gcc"
# Use intrinsics or assembly code for key routines
CONFIG_RTE_FORCE_INTRINSICS=n
# Machine forces strict alignment constraints.
CONFIG_RTE_ARCH_STRICT_ALIGN=n
# Compile to share library
CONFIG_RTE_BUILD_SHARED_LIB=n
# Use newest code breaking previous ABI
CONFIG_RTE_NEXT_ABI=n
# Major ABI to overwrite library specific LIBABIVER
CONFIG_RTE_MAJOR_ABI=
# Machine's cache line size
CONFIG_RTE_CACHE_LINE_SIZE=64
# Compile Environment Abstraction Layer
CONFIG_RTE_LIBRTE_EAL=y
CONFIG_RTE_MAX_LCORE=128
CONFIG_RTE_MAX_NUMA_NODES=8
CONFIG_RTE_MAX_MEMSEG=256
CONFIG_RTE_MAX_MEMZONE=2560
CONFIG_RTE_MAX_TAILQ=32
CONFIG_RTE_ENABLE_ASSERT=n
CONFIG_RTE_LOG_LEVEL=RTE_LOG_INFO
CONFIG_RTE_LOG_DP_LEVEL=RTE_LOG_INFO
CONFIG_RTE_LOG_HISTORY=256
CONFIG_RTE_BACKTRACE=y
CONFIG_RTE_LIBEAL_USE_HPET=n
CONFIG_RTE_EAL_ALLOW_INV_SOCKET_ID=n
CONFIG_RTE_EAL_ALWAYS_PANIC_ON_ERROR=n
CONFIG_RTE_EAL_IGB_UIO=n
CONFIG_RTE_EAL_VFIO=y
CONFIG_RTE_MALLOC_DEBUG=n
CONFIG_RTE_EAL_NUMA_AWARE_HUGEPAGES=y
# Recognize/ignore architecture we compile for. AVX/AVX512 CPU flags for performance/power testing.
# AVX512 is marked as experimental for now, will enable it after enough
# field test and possible optimization.
CONFIG_RTE_ENABLE_AVX=y
CONFIG_RTE_ENABLE_AVX512=n
# Default driver path (or "" to disable)
CONFIG_RTE_EAL_PMD_PATH=""
# Compile Environment Abstraction Layer to support Vmware TSC map
CONFIG_RTE_LIBRTE_EAL_VMWARE_TSC_MAP_SUPPORT=y
# Compile architecture we compile for. PCI library
CONFIG_RTE_LIBRTE_PCI=y
# Compile architecture we compile for. argument parser library
CONFIG_RTE_LIBRTE_KVARGS=y
# Compile generic ethernet library
CONFIG_RTE_LIBRTE_ETHER=y
CONFIG_RTE_LIBRTE_ETHDEV_DEBUG=n
CONFIG_RTE_MAX_ETHPORTS=32
CONFIG_RTE_MAX_QUEUES_PER_PORT=1024
CONFIG_RTE_LIBRTE_IEEE1588=n
CONFIG_RTE_ETHDEV_QUEUE_STAT_CNTRS=16
CONFIG_RTE_ETHDEV_RXTX_CALLBACKS=y
CONFIG_RTE_ETHDEV_PROFILE_ITT_WASTED_RX_ITERATIONS=n
# Turn off Tx preparation stage
# Warning: rte_eth_tx_prepare() can be safely disabled only if using a
# driver which do not implement any Tx preparation.
CONFIG_RTE_ETHDEV_TX_PREPARE_NOOP=n
# Compile PCI bus driver
CONFIG_RTE_LIBRTE_PCI_BUS=y
# Compile architecture we compile for. vdev bus
CONFIG_RTE_LIBRTE_VDEV_BUS=y
# Compile burst-oriented Amazon ENA PMD driver
CONFIG_RTE_LIBRTE_ENA_PMD=n
CONFIG_RTE_LIBRTE_ENA_DEBUG_RX=n
CONFIG_RTE_LIBRTE_ENA_DEBUG_TX=n
CONFIG_RTE_LIBRTE_ENA_DEBUG_TX_FREE=n
CONFIG_RTE_LIBRTE_ENA_DEBUG_DRIVER=n
CONFIG_RTE_LIBRTE_ENA_COM_DEBUG=n
# Compile burst-oriented IGB & EM PMD drivers
CONFIG_RTE_LIBRTE_EM_PMD=n
CONFIG_RTE_LIBRTE_IGB_PMD=y
CONFIG_RTE_LIBRTE_E1000_DEBUG_INIT=n
CONFIG_RTE_LIBRTE_E1000_DEBUG_RX=n
CONFIG_RTE_LIBRTE_E1000_DEBUG_TX=n
CONFIG_RTE_LIBRTE_E1000_DEBUG_TX_FREE=n
CONFIG_RTE_LIBRTE_E1000_DEBUG_DRIVER=n
CONFIG_RTE_LIBRTE_E1000_PF_DISABLE_STRIP_CRC=n
# Compile burst-oriented IXGBE PMD driver
CONFIG_RTE_LIBRTE_IXGBE_PMD=y
CONFIG_RTE_LIBRTE_IXGBE_DEBUG_INIT=n
CONFIG_RTE_LIBRTE_IXGBE_DEBUG_RX=n
CONFIG_RTE_LIBRTE_IXGBE_DEBUG_TX=n
CONFIG_RTE_LIBRTE_IXGBE_DEBUG_TX_FREE=n
CONFIG_RTE_LIBRTE_IXGBE_DEBUG_DRIVER=n
CONFIG_RTE_LIBRTE_IXGBE_PF_DISABLE_STRIP_CRC=n
CONFIG_RTE_IXGBE_INC_VECTOR=y
CONFIG_RTE_LIBRTE_IXGBE_BYPASS=n
# Compile burst-oriented I40E PMD driver
CONFIG_RTE_LIBRTE_I40E_PMD=y
CONFIG_RTE_LIBRTE_I40E_DEBUG_RX=n
CONFIG_RTE_LIBRTE_I40E_DEBUG_TX=n
CONFIG_RTE_LIBRTE_I40E_DEBUG_TX_FREE=n
CONFIG_RTE_LIBRTE_I40E_RX_ALLOW_BULK_ALLOC=y
CONFIG_RTE_LIBRTE_I40E_INC_VECTOR=y
CONFIG_RTE_LIBRTE_I40E_16BYTE_RX_DESC=n
CONFIG_RTE_LIBRTE_I40E_QUEUE_NUM_PER_PF=64
CONFIG_RTE_LIBRTE_I40E_QUEUE_NUM_PER_VF=4
CONFIG_RTE_LIBRTE_I40E_QUEUE_NUM_PER_VM=4
# interval up to 8160 us, aligned to 2 (or default value)
CONFIG_RTE_LIBRTE_I40E_ITR_INTERVAL=-1
# Compile burst-oriented FM10K PMD
CONFIG_RTE_LIBRTE_FM10K_PMD=n
CONFIG_RTE_LIBRTE_FM10K_DEBUG_INIT=n
CONFIG_RTE_LIBRTE_FM10K_DEBUG_RX=n
CONFIG_RTE_LIBRTE_FM10K_DEBUG_TX=n
CONFIG_RTE_LIBRTE_FM10K_DEBUG_TX_FREE=n
CONFIG_RTE_LIBRTE_FM10K_DEBUG_DRIVER=n
CONFIG_RTE_LIBRTE_FM10K_RX_OLFLAGS_ENABLE=y
CONFIG_RTE_LIBRTE_FM10K_INC_VECTOR=y
# Compile burst-oriented Mellanox ConnectX-3 (MLX4) PMD
CONFIG_RTE_LIBRTE_MLX4_PMD=n
CONFIG_RTE_LIBRTE_MLX4_DEBUG=n
CONFIG_RTE_LIBRTE_MLX4_DEBUG_BROKEN_VERBS=n
CONFIG_RTE_LIBRTE_MLX4_TX_MP_CACHE=8
# Compile burst-oriented Mellanox ConnectX-4 & ConnectX-5 (MLX5) PMD
CONFIG_RTE_LIBRTE_MLX5_PMD=n
CONFIG_RTE_LIBRTE_MLX5_DEBUG=n
CONFIG_RTE_LIBRTE_MLX5_TX_MP_CACHE=8
# Compile burst-oriented Broadcom PMD driver
CONFIG_RTE_LIBRTE_BNX2X_PMD=n
CONFIG_RTE_LIBRTE_BNX2X_DEBUG=n
CONFIG_RTE_LIBRTE_BNX2X_DEBUG_INIT=n
CONFIG_RTE_LIBRTE_BNX2X_DEBUG_RX=n
CONFIG_RTE_LIBRTE_BNX2X_DEBUG_TX=n
CONFIG_RTE_LIBRTE_BNX2X_MF_SUPPORT=n
CONFIG_RTE_LIBRTE_BNX2X_DEBUG_PERIODIC=n
# Compile burst-oriented Chelsio Terminator (CXGBE) PMD
CONFIG_RTE_LIBRTE_CXGBE_PMD=n
CONFIG_RTE_LIBRTE_CXGBE_DEBUG=n
CONFIG_RTE_LIBRTE_CXGBE_DEBUG_REG=n
CONFIG_RTE_LIBRTE_CXGBE_DEBUG_MBOX=n
CONFIG_RTE_LIBRTE_CXGBE_DEBUG_TX=n
CONFIG_RTE_LIBRTE_CXGBE_DEBUG_RX=n
CONFIG_RTE_LIBRTE_CXGBE_TPUT=y
# Compile burst-oriented Cisco ENIC PMD driver
CONFIG_RTE_LIBRTE_ENIC_PMD=y
CONFIG_RTE_LIBRTE_ENIC_DEBUG=n
CONFIG_RTE_LIBRTE_ENIC_DEBUG_FLOW=n
# Compile burst-oriented Netronome NFP PMD driver
CONFIG_RTE_LIBRTE_NFP_PMD=n
CONFIG_RTE_LIBRTE_NFP_DEBUG=n
# Compile Marvell PMD driver
CONFIG_RTE_LIBRTE_MRVL_PMD=n
# Compile burst-oriented Broadcom BNXT PMD driver
CONFIG_RTE_LIBRTE_BNXT_PMD=n
# Compile burst-oriented Solarflare libefx-based PMD
CONFIG_RTE_LIBRTE_SFC_EFX_PMD=n
CONFIG_RTE_LIBRTE_SFC_EFX_DEBUG=n
# Compile SOFTNIC PMD
CONFIG_RTE_LIBRTE_PMD_SOFTNIC=y
# Compile software PMD backed by SZEDATA2 device
CONFIG_RTE_LIBRTE_PMD_SZEDATA2=n
# Defines firmware type address space.
# See documentation for supported values.
# Other values raise compile time error.
CONFIG_RTE_LIBRTE_PMD_SZEDATA2_AS=0
# Compile burst-oriented Cavium Thunderx NICVF PMD driver
CONFIG_RTE_LIBRTE_THUNDERX_NICVF_PMD=n
CONFIG_RTE_LIBRTE_THUNDERX_NICVF_DEBUG_INIT=n
CONFIG_RTE_LIBRTE_THUNDERX_NICVF_DEBUG_RX=n
CONFIG_RTE_LIBRTE_THUNDERX_NICVF_DEBUG_TX=n
CONFIG_RTE_LIBRTE_THUNDERX_NICVF_DEBUG_DRIVER=n
CONFIG_RTE_LIBRTE_THUNDERX_NICVF_DEBUG_MBOX=n
# Compile burst-oriented Cavium LiquidIO PMD driver
CONFIG_RTE_LIBRTE_LIO_PMD=n
CONFIG_RTE_LIBRTE_LIO_DEBUG_DRIVER=n
CONFIG_RTE_LIBRTE_LIO_DEBUG_INIT=n
CONFIG_RTE_LIBRTE_LIO_DEBUG_RX=n
CONFIG_RTE_LIBRTE_LIO_DEBUG_TX=n
CONFIG_RTE_LIBRTE_LIO_DEBUG_MBOX=n
CONFIG_RTE_LIBRTE_LIO_DEBUG_REGS=n
# NXP DPAA Bus
CONFIG_RTE_LIBRTE_DPAA_BUS=n
CONFIG_RTE_LIBRTE_DPAA_MEMPOOL=n
CONFIG_RTE_LIBRTE_DPAA_PMD=n
# Compile burst-oriented Cavium OCTEONTX network PMD driver
CONFIG_RTE_LIBRTE_OCTEONTX_PMD=n
CONFIG_RTE_LIBRTE_OCTEONTX_DEBUG_INIT=n
CONFIG_RTE_LIBRTE_OCTEONTX_DEBUG_RX=n
CONFIG_RTE_LIBRTE_OCTEONTX_DEBUG_TX=n
CONFIG_RTE_LIBRTE_OCTEONTX_DEBUG_DRIVER=n
CONFIG_RTE_LIBRTE_OCTEONTX_DEBUG_MBOX=n
# Compile NXP DPAA2 FSL-MC Bus
CONFIG_RTE_LIBRTE_FSLMC_BUS=n
# Compile Support Libraries for NXP DPAA2
CONFIG_RTE_LIBRTE_DPAA2_MEMPOOL=n
CONFIG_RTE_LIBRTE_DPAA2_USE_PHYS_IOVA=y
# Compile burst-oriented NXP DPAA2 PMD driver
CONFIG_RTE_LIBRTE_DPAA2_PMD=n
CONFIG_RTE_LIBRTE_DPAA2_DEBUG_INIT=n
CONFIG_RTE_LIBRTE_DPAA2_DEBUG_DRIVER=n
CONFIG_RTE_LIBRTE_DPAA2_DEBUG_RX=n
CONFIG_RTE_LIBRTE_DPAA2_DEBUG_TX=n
CONFIG_RTE_LIBRTE_DPAA2_DEBUG_TX_FREE=n
# Compile burst-oriented VIRTIO PMD driver
CONFIG_RTE_LIBRTE_VIRTIO_PMD=y
CONFIG_RTE_LIBRTE_VIRTIO_DEBUG_INIT=n
CONFIG_RTE_LIBRTE_VIRTIO_DEBUG_RX=n
CONFIG_RTE_LIBRTE_VIRTIO_DEBUG_TX=n
CONFIG_RTE_LIBRTE_VIRTIO_DEBUG_DRIVER=n
CONFIG_RTE_LIBRTE_VIRTIO_DEBUG_DUMP=n
# Compile virtio device emulation inside virtio PMD driver
CONFIG_RTE_VIRTIO_USER=n
# Compile burst-oriented VMXNET3 PMD driver
CONFIG_RTE_LIBRTE_VMXNET3_PMD=n
CONFIG_RTE_LIBRTE_VMXNET3_DEBUG_INIT=n
CONFIG_RTE_LIBRTE_VMXNET3_DEBUG_RX=n
CONFIG_RTE_LIBRTE_VMXNET3_DEBUG_TX=n
CONFIG_RTE_LIBRTE_VMXNET3_DEBUG_TX_FREE=n
CONFIG_RTE_LIBRTE_VMXNET3_DEBUG_DRIVER=n
# Compile example software rings based PMD
CONFIG_RTE_LIBRTE_PMD_RING=y
CONFIG_RTE_PMD_RING_MAX_RX_RINGS=16
CONFIG_RTE_PMD_RING_MAX_TX_RINGS=16
# Compile software PMD backed by PCAP files
CONFIG_RTE_LIBRTE_PMD_PCAP=n
# Compile link bonding PMD library
CONFIG_RTE_LIBRTE_PMD_BOND=n
CONFIG_RTE_LIBRTE_BOND_DEBUG_ALB=n
CONFIG_RTE_LIBRTE_BOND_DEBUG_ALB_L1=n
# QLogic 10G/25G/40G/50G/100G PMD
CONFIG_RTE_LIBRTE_QEDE_PMD=n
CONFIG_RTE_LIBRTE_QEDE_DEBUG_INIT=n
CONFIG_RTE_LIBRTE_QEDE_DEBUG_INFO=n
CONFIG_RTE_LIBRTE_QEDE_DEBUG_DRIVER=n
CONFIG_RTE_LIBRTE_QEDE_DEBUG_TX=n
CONFIG_RTE_LIBRTE_QEDE_DEBUG_RX=n
CONFIG_RTE_LIBRTE_QEDE_VF_TX_SWITCH=y
#Provides abs path/name of architecture we compile for. firmware file.
#Empty string denotes driver will use default firmware
CONFIG_RTE_LIBRTE_QEDE_FW=""
# Compile software PMD backed by AF_PACKET sockets (Linux only)
CONFIG_RTE_LIBRTE_PMD_AF_PACKET=n
# Compile ARK PMD
CONFIG_RTE_LIBRTE_ARK_PMD=n
CONFIG_RTE_LIBRTE_ARK_PAD_TX=y
CONFIG_RTE_LIBRTE_ARK_DEBUG_RX=n
CONFIG_RTE_LIBRTE_ARK_DEBUG_TX=n
CONFIG_RTE_LIBRTE_ARK_DEBUG_STATS=n
CONFIG_RTE_LIBRTE_ARK_DEBUG_TRACE=n
# Compile WRS accelerated virtual port (AVP) guest PMD driver
CONFIG_RTE_LIBRTE_AVP_PMD=n
CONFIG_RTE_LIBRTE_AVP_DEBUG_RX=n
CONFIG_RTE_LIBRTE_AVP_DEBUG_TX=n
CONFIG_RTE_LIBRTE_AVP_DEBUG_DRIVER=y
CONFIG_RTE_LIBRTE_AVP_DEBUG_BUFFERS=n
# Compile architecture we compile for. TAP PMD
# It is enabled by default for Linux only.
CONFIG_RTE_LIBRTE_PMD_TAP=n
# Compile null PMD
CONFIG_RTE_LIBRTE_PMD_NULL=n
# Compile fail-safe PMD
CONFIG_RTE_LIBRTE_PMD_FAILSAFE=y
# Do prefetch of packet data within PMD driver receive function
CONFIG_RTE_PMD_PACKET_PREFETCH=y
# Compile generic crypto device library
CONFIG_RTE_LIBRTE_CRYPTODEV=n
CONFIG_RTE_LIBRTE_CRYPTODEV_DEBUG=n
CONFIG_RTE_CRYPTO_MAX_DEVS=64
CONFIG_RTE_CRYPTODEV_NAME_LEN=64
# Compile PMD for ARMv8 Crypto device
CONFIG_RTE_LIBRTE_PMD_ARMV8_CRYPTO=n
CONFIG_RTE_LIBRTE_PMD_ARMV8_CRYPTO_DEBUG=n
# Compile NXP DPAA2 crypto sec driver for CAAM HW
CONFIG_RTE_LIBRTE_PMD_DPAA2_SEC=n
CONFIG_RTE_LIBRTE_DPAA2_SEC_DEBUG_INIT=n
CONFIG_RTE_LIBRTE_DPAA2_SEC_DEBUG_DRIVER=n
CONFIG_RTE_LIBRTE_DPAA2_SEC_DEBUG_RX=n
# NXP DPAA caam - crypto driver
CONFIG_RTE_LIBRTE_PMD_DPAA_SEC=n
CONFIG_RTE_LIBRTE_DPAA_SEC_DEBUG_INIT=n
CONFIG_RTE_LIBRTE_DPAA_SEC_DEBUG_DRIVER=n
CONFIG_RTE_LIBRTE_DPAA_SEC_DEBUG_RX=n
# Compile PMD for QuickAssist based devices
CONFIG_RTE_LIBRTE_PMD_QAT=n
CONFIG_RTE_LIBRTE_PMD_QAT_DEBUG_INIT=n
CONFIG_RTE_LIBRTE_PMD_QAT_DEBUG_TX=n
CONFIG_RTE_LIBRTE_PMD_QAT_DEBUG_RX=n
CONFIG_RTE_LIBRTE_PMD_QAT_DEBUG_DRIVER=n
# Number of sessions to create in architecture we compile for. session memory pool
# on a single QuickAssist device.
CONFIG_RTE_QAT_PMD_MAX_NB_SESSIONS=2048
# Compile PMD for AESNI backed device
CONFIG_RTE_LIBRTE_PMD_AESNI_MB=n
CONFIG_RTE_LIBRTE_PMD_AESNI_MB_DEBUG=n
# Compile PMD for Software backed device
CONFIG_RTE_LIBRTE_PMD_OPENSSL=n
CONFIG_RTE_LIBRTE_PMD_OPENSSL_DEBUG=n
# Compile PMD for AESNI GCM device
CONFIG_RTE_LIBRTE_PMD_AESNI_GCM=n
CONFIG_RTE_LIBRTE_PMD_AESNI_GCM_DEBUG=n
# Compile PMD for SNOW 3G device
CONFIG_RTE_LIBRTE_PMD_SNOW3G=n
CONFIG_RTE_LIBRTE_PMD_SNOW3G_DEBUG=n
# Compile PMD for KASUMI device
CONFIG_RTE_LIBRTE_PMD_KASUMI=n
CONFIG_RTE_LIBRTE_PMD_KASUMI_DEBUG=n
# Compile PMD for ZUC device
CONFIG_RTE_LIBRTE_PMD_ZUC=n
CONFIG_RTE_LIBRTE_PMD_ZUC_DEBUG=n
# Compile PMD for Crypto Scheduler device
CONFIG_RTE_LIBRTE_PMD_CRYPTO_SCHEDULER=n
CONFIG_RTE_LIBRTE_PMD_CRYPTO_SCHEDULER_DEBUG=n
# Compile PMD for NULL Crypto device
CONFIG_RTE_LIBRTE_PMD_NULL_CRYPTO=n
# Compile PMD for Marvell Crypto device
CONFIG_RTE_LIBRTE_PMD_MRVL_CRYPTO=n
CONFIG_RTE_LIBRTE_PMD_MRVL_CRYPTO_DEBUG=n
# Compile generic security library
CONFIG_RTE_LIBRTE_SECURITY=n
# Compile generic event device library
CONFIG_RTE_LIBRTE_EVENTDEV=y
CONFIG_RTE_LIBRTE_EVENTDEV_DEBUG=n
CONFIG_RTE_EVENT_MAX_DEVS=16
CONFIG_RTE_EVENT_MAX_QUEUES_PER_DEV=64
# Compile PMD for skeleton event device
CONFIG_RTE_LIBRTE_PMD_SKELETON_EVENTDEV=n
CONFIG_RTE_LIBRTE_PMD_SKELETON_EVENTDEV_DEBUG=n
# Compile PMD for software event device
CONFIG_RTE_LIBRTE_PMD_SW_EVENTDEV=n
CONFIG_RTE_LIBRTE_PMD_SW_EVENTDEV_DEBUG=n
# Compile PMD for octeontx sso event device
CONFIG_RTE_LIBRTE_PMD_OCTEONTX_SSOVF=n
CONFIG_RTE_LIBRTE_PMD_OCTEONTX_SSOVF_DEBUG=n
# Compile librte_ring
CONFIG_RTE_LIBRTE_RING=y
# Compile librte_mempool
CONFIG_RTE_LIBRTE_MEMPOOL=y
CONFIG_RTE_MEMPOOL_CACHE_MAX_SIZE=512
CONFIG_RTE_LIBRTE_MEMPOOL_DEBUG=n
# Compile Mempool drivers
CONFIG_RTE_DRIVER_MEMPOOL_RING=y
CONFIG_RTE_DRIVER_MEMPOOL_STACK=y
# Compile PMD for octeontx fpa mempool device
CONFIG_RTE_LIBRTE_OCTEONTX_MEMPOOL=y
CONFIG_RTE_LIBRTE_OCTEONTX_MEMPOOL_DEBUG=n
# Compile librte_mbuf
CONFIG_RTE_LIBRTE_MBUF=y
CONFIG_RTE_LIBRTE_MBUF_DEBUG=n
CONFIG_RTE_MBUF_DEFAULT_MEMPOOL_OPS="ring_mp_mc"
CONFIG_RTE_MBUF_REFCNT_ATOMIC=y
CONFIG_RTE_PKTMBUF_HEADROOM=128
# Compile librte_timer
CONFIG_RTE_LIBRTE_TIMER=n
CONFIG_RTE_LIBRTE_TIMER_DEBUG=n
# Compile librte_cfgfile
CONFIG_RTE_LIBRTE_CFGFILE=n
# Compile librte_cmdline
CONFIG_RTE_LIBRTE_CMDLINE=y
CONFIG_RTE_LIBRTE_CMDLINE_DEBUG=n
# Compile librte_hash
CONFIG_RTE_LIBRTE_HASH=y
CONFIG_RTE_LIBRTE_HASH_DEBUG=n
# Compile librte_efd
CONFIG_RTE_LIBRTE_EFD=y
# Compile librte_member
CONFIG_RTE_LIBRTE_MEMBER=y
# Compile librte_jobstats
CONFIG_RTE_LIBRTE_JOBSTATS=n
# Compile architecture we compile for. device metrics library
CONFIG_RTE_LIBRTE_METRICS=y
# Compile architecture we compile for. bitrate statistics library
CONFIG_RTE_LIBRTE_BITRATE=y
# Compile architecture we compile for. latency statistics library
CONFIG_RTE_LIBRTE_LATENCY_STATS=y
# Compile librte_lpm
CONFIG_RTE_LIBRTE_LPM=n
CONFIG_RTE_LIBRTE_LPM_DEBUG=n
# Compile librte_acl
CONFIG_RTE_LIBRTE_ACL=n
CONFIG_RTE_LIBRTE_ACL_DEBUG=n
# Compile librte_power
CONFIG_RTE_LIBRTE_POWER=n
CONFIG_RTE_LIBRTE_POWER_DEBUG=n
CONFIG_RTE_MAX_LCORE_FREQS=64
# Compile librte_net
CONFIG_RTE_LIBRTE_NET=y
# Compile librte_ip_frag
CONFIG_RTE_LIBRTE_IP_FRAG=y
CONFIG_RTE_LIBRTE_IP_FRAG_DEBUG=n
CONFIG_RTE_LIBRTE_IP_FRAG_MAX_FRAG=4
CONFIG_RTE_LIBRTE_IP_FRAG_TBL_STAT=n
# Compile GRO library
CONFIG_RTE_LIBRTE_GRO=y
# Compile GSO library
CONFIG_RTE_LIBRTE_GSO=y
# Compile librte_meter
CONFIG_RTE_LIBRTE_METER=y
# Compile librte_classify
CONFIG_RTE_LIBRTE_FLOW_CLASSIFY=n
# Compile librte_sched
CONFIG_RTE_LIBRTE_SCHED=y
CONFIG_RTE_SCHED_DEBUG=n
CONFIG_RTE_SCHED_RED=n
CONFIG_RTE_SCHED_COLLECT_STATS=n
CONFIG_RTE_SCHED_SUBPORT_TC_OV=n
CONFIG_RTE_SCHED_PORT_N_GRINDERS=8
CONFIG_RTE_SCHED_VECTOR=n
# Compile architecture we compile for. distributor library
CONFIG_RTE_LIBRTE_DISTRIBUTOR=n
# Compile architecture we compile for. reorder library
CONFIG_RTE_LIBRTE_REORDER=n
# Compile librte_port
CONFIG_RTE_LIBRTE_PORT=n
CONFIG_RTE_PORT_STATS_COLLECT=n
CONFIG_RTE_PORT_PCAP=n
# Compile librte_table
CONFIG_RTE_LIBRTE_TABLE=n
CONFIG_RTE_TABLE_STATS_COLLECT=n
# Compile librte_pipeline
CONFIG_RTE_LIBRTE_PIPELINE=n
CONFIG_RTE_PIPELINE_STATS_COLLECT=n
# Compile librte_kni
CONFIG_RTE_LIBRTE_KNI=n
CONFIG_RTE_LIBRTE_PMD_KNI=n
CONFIG_RTE_KNI_KMOD=n
CONFIG_RTE_KNI_KMOD_ETHTOOL=n
CONFIG_RTE_KNI_PREEMPT_DEFAULT=y
# Compile architecture we compile for. pdump library
CONFIG_RTE_LIBRTE_PDUMP=y
# Compile vhost user library
CONFIG_RTE_LIBRTE_VHOST=y
CONFIG_RTE_LIBRTE_VHOST_NUMA=y
CONFIG_RTE_LIBRTE_VHOST_DEBUG=n
# Compile vhost PMD
# To compile, CONFIG_RTE_LIBRTE_VHOST should be enabled.
CONFIG_RTE_LIBRTE_PMD_VHOST=n
# Compile architecture we compile for. test application
CONFIG_RTE_APP_TEST=y
CONFIG_RTE_APP_TEST_RESOURCE_TAR=n
# Compile architecture we compile for. PMD test application
CONFIG_RTE_TEST_PMD=n
CONFIG_RTE_TEST_PMD_RECORD_CORE_CYCLES=n
CONFIG_RTE_TEST_PMD_RECORD_BURST_STATS=n
# Compile architecture we compile for. crypto performance application
CONFIG_RTE_APP_CRYPTO_PERF=y
# Compile architecture we compile for. eventdev application
CONFIG_RTE_APP_EVENTDEV=y
CONFIG_RTE_EXEC_ENV_LINUXAPP=y
CONFIG_RTE_ARCH_X86_64=y
CONFIG_RTE_ARCH_X86=y
CONFIG_RTE_ARCH_64=y
CONFIG_RTE_TOOLCHAIN_GCC=y
CONFIG_RTE_LIBRTE_PMD_XENVIRT=n
