--- thin-provisioning-tools-0.4.1/man8/era_restore.8.orig	2014-10-28 14:24:43.356272471 +0100
+++ thin-provisioning-tools-0.4.1/man8/era_restore.8	2014-10-28 14:28:56.358133852 +0100
@@ -0,0 +1,63 @@
+.TH ERA_RESTORE 8 "Thin Provisioning Tools" "Red Hat, Inc." \" -*- nroff -*-
+.SH NAME
+era_restore \- restore era metadata file to device or file
+
+.SH SYNOPSIS
+.B era_restore
+.RB [ options ]
+.RB -i
+.I {device|file}
+.RB -o
+.I {device|file}
+
+.SH DESCRIPTION
+.B era_restore
+restores binary era metadata created by the
+respective device-mapper target dumped into an XML formatted (see
+.BR era_dump(8) )
+.I file
+, which optionally can be preprocessed before the restore to another
+.I device
+or
+.I file.
+If restored to a metadata
+.I device
+, the metadata can be processed by the device-mapper target.
+
+.IP "\fB\-q, \-\-quiet\fP"
+Suppress output messages, return only exit code.
+
+.IP "\fB\-i, \-\-input\fP \fI{device|file}\fP"
+Input file or device with metadata.
+
+.IP "\fB\-o, \-\-output\fP \fI{device|file}\fP"
+Output file or device.
+
+.IP "\fB\-h, \-\-help\fP"
+Print help and exit.
+
+.IP "\fB\-V, \-\-version\fP"
+Output version information and exit.
+
+.SH EXAMPLE
+Restores the XML formatted era metadata on file
+.B metadata
+to logical volume /dev/vg/metadata for further processing by the
+respective device-mapper target:
+.sp
+.B era_restore -i metadata -o /dev/vg/metadata
+
+.SH DIAGNOSTICS
+.B era_restore
+returns an exit code of 0 for success or 1 for error.
+
+.SH SEE ALSO
+.B era_check(8)
+.B era_dump(8)
+.B era_invaidate(8)
+.B era_restore(8)
+
+.SH AUTHOR
+Joe Thornber <ejt@redhat.com>
+.br
+Heinz Mauelshagen <HeinzM@RedHat.com>
--- thin-provisioning-tools-0.4.1/man8/cache_metadata_size.8.orig	2014-10-28 14:31:49.116087709 +0100
+++ thin-provisioning-tools-0.4.1/man8/cache_metadata_size.8	2014-10-28 14:50:29.337238755 +0100
@@ -0,0 +1,47 @@
+.TH CACHE_METADATA_SIZE 8 "Thin Provisioning Tools" "Red Hat, Inc." \" -*- nroff -*-
+.SH NAME
+cache_metadata_size \- cache metadata device/file size calculator.
+
+.SH SYNOPSIS
+.B cache_metadata_size
+.RB [ options ]
+
+.SH DESCRIPTION
+.B cache_metadata_size
+calculates the size of the cache metadata based on the block size
+of the cache device and the cache block size.
+All relates to the size of the fast device (eg, SSD), rather
+than the whole cached (i.e. origin) device.
+
+.IP "\fB\\-\-block\-size <sectors>\fP
+Block size of cache in units of sectors.
+
+.IP "\fB\\-\-device\-size <sectors>\fP
+Device size of the cache device in units of sectors.
+
+.IP "\fB\\-\-nr\-blocks <natural>\fP
+Capacity of the cache in number of blocks.
+
+.IP "\fB\-h, \-\-help\fP"
+Print help and exit.
+
+.IP "\fB\-V, \-\-version\fP"
+Output version information and exit.
+
+.SH EXAMPLES
+Calculates the cache metadata device size for block size 256 sectors.and device size of 2GiB
+.sp
+.B cache_metadata_size --block-size 256 --device-size $((2*1024*1024))
+
+.SH DIAGNOSTICS
+.B cache_metadata_size
+returns an exit code of 0 for success or 1 for error.
+
+.SH SEE ALSO
+.B cache_check(8)
+.B cache_dump(8)
+.B cache_repair(8)
+.B cache_restore(8)
+
+.SH AUTHOR
+Heinz Mauelshagen <HeinzM@RedHat.com>
