From dd0a4f1120118f08a4d760ceec511238321779f8 Mon Sep 17 00:00:00 2001
From: Vladimir Serbinenko <phcoder@gmail.com>
Date: Fri, 28 Feb 2014 10:07:11 +0100
Subject: [PATCH 064/237] * grub-core/kern/i386/pc/mmap.c: Fallback to EISA
 memory map if E820 failed to return any regions.

---
 ChangeLog                     |  5 +++++
 grub-core/kern/i386/pc/mmap.c | 40 +++++++++++++++++++++-------------------
 2 files changed, 26 insertions(+), 19 deletions(-)

diff --git a/ChangeLog b/ChangeLog
index 6ed6cf4..97cf57e 100644
--- a/ChangeLog
+++ b/ChangeLog
@@ -1,5 +1,10 @@
 2014-02-28  Vladimir Serbinenko  <phcoder@gmail.com>
 
+	* grub-core/kern/i386/pc/mmap.c: Fallback to EISA memory map
+	if E820 failed to return any regions.
+
+2014-02-28  Vladimir Serbinenko  <phcoder@gmail.com>
+
 	* grub-core/mmap/i386/uppermem.c (lower_hook) [COREBOOT]: Ignore low
 	tables for low memory calculations.
 
diff --git a/grub-core/kern/i386/pc/mmap.c b/grub-core/kern/i386/pc/mmap.c
index 8009e83..f1375f3 100644
--- a/grub-core/kern/i386/pc/mmap.c
+++ b/grub-core/kern/i386/pc/mmap.c
@@ -141,33 +141,35 @@ grub_get_mmap_entry (struct grub_machine_mmap_entry *entry,
 grub_err_t
 grub_machine_mmap_iterate (grub_memory_hook_t hook, void *hook_data)
 {
-  grub_uint32_t cont;
+  grub_uint32_t cont = 0;
   struct grub_machine_mmap_entry *entry
     = (struct grub_machine_mmap_entry *) GRUB_MEMORY_MACHINE_SCRATCH_ADDR;
+  int e820_works = 0;
 
-  grub_memset (entry, 0, sizeof (entry));
+  while (1)
+    {
+      grub_memset (entry, 0, sizeof (entry));
 
-  /* Check if grub_get_mmap_entry works.  */
-  cont = grub_get_mmap_entry (entry, 0);
+      cont = grub_get_mmap_entry (entry, cont);
 
-  if (entry->size)
-    do
-      {
-	if (hook (entry->addr, entry->len,
-		  /* GRUB mmaps have been defined to match with the E820 definition.
-		     Therefore, we can just pass type through.  */
-		  entry->type, hook_data))
-	  break;
+      if (!entry->size)
+	break;
 
-	if (! cont)
-	  break;
+      if (entry->len)
+	e820_works = 1;
+      if (entry->len
+	  && hook (entry->addr, entry->len,
+		   /* GRUB mmaps have been defined to match with
+		      the E820 definition.
+		      Therefore, we can just pass type through.  */
+		   entry->type, hook_data))
+	break;
 
-	grub_memset (entry, 0, sizeof (entry));
+      if (! cont)
+	break;
+    }
 
-	cont = grub_get_mmap_entry (entry, cont);
-      }
-    while (entry->size);
-  else
+  if (!e820_works)
     {
       grub_uint32_t eisa_mmap = grub_get_eisa_mmap ();
 
-- 
2.9.3

