From 5fc42eeb85e2971ea777fbe2c95e2b0d384bb86d Mon Sep 17 00:00:00 2001
From: Mike Gilbert <floppym@gentoo.org>
Date: Sun, 26 Jan 2014 02:56:04 +0100
Subject: [PATCH 047/237] grub-install: support for partitioned partx loop
 devices.

	* grub-core/osdep/linux/getroot.c (grub_util_part_to_disk): Detect
	/dev/loopX as being the parent of /dev/loopXpY.
---
 ChangeLog                       |  7 +++++++
 grub-core/osdep/linux/getroot.c | 13 +++++++++++++
 2 files changed, 20 insertions(+)

diff --git a/ChangeLog b/ChangeLog
index 67b4d5c..bbec1e7 100644
--- a/ChangeLog
+++ b/ChangeLog
@@ -1,3 +1,10 @@
+2014-01-26  Mike Gilbert <floppym@gentoo.org>
+
+	grub-install: support for partitioned partx loop devices.
+
+	* grub-core/osdep/linux/getroot.c (grub_util_part_to_disk): Detect
+	/dev/loopX as being the parent of /dev/loopXpY.
+
 2014-01-26  Vladimir Serbinenko  <phcoder@gmail.com>
 
 	* grub-core/term/serial.c (grub_serial_register): Fix invalid free.
diff --git a/grub-core/osdep/linux/getroot.c b/grub-core/osdep/linux/getroot.c
index 772de0a..19581d3 100644
--- a/grub-core/osdep/linux/getroot.c
+++ b/grub-core/osdep/linux/getroot.c
@@ -883,6 +883,19 @@ grub_util_part_to_disk (const char *os_dev, struct stat *st,
 	  *pp = '\0';
 	  return path;
 	}
+
+      /* If this is a loop device */
+      if ((strncmp ("loop", p, 4) == 0) && p[4] >= '0' && p[4] <= '9')
+	{
+	  char *pp = p + 4;
+	  while (*pp >= '0' && *pp <= '9')
+	    pp++;
+	  if (*pp == 'p')
+	    *is_part = 1;
+	  /* /dev/loop[0-9]+p[0-9]* */
+	  *pp = '\0';
+	  return path;
+	}
     }
 
   return path;
-- 
2.9.3

