From a7f0e26a47e0caa465cf757de74574656e5cabd1 Mon Sep 17 00:00:00 2001
From: Aaron Armstrong Skomra <skomra@gmail.com>
Date: Wed, 1 Mar 2017 10:37:15 -0800
Subject: [PATCH libwacom] data: add support for Cintiq Pro 13 & 16

These devices have no buttons, hence no .svg files.

Signed-off-by: Aaron Armstrong Skomra <aaron.skomra@wacom.com>
Signed-off-by: Peter Hutterer <peter.hutterer@who-t.net>
---
 data/cintiq-pro-13.tablet | 45 +++++++++++++++++++++++++++++++++++++++++++++
 data/cintiq-pro-16.tablet | 45 +++++++++++++++++++++++++++++++++++++++++++++
 2 files changed, 90 insertions(+)
 create mode 100644 data/cintiq-pro-13.tablet
 create mode 100644 data/cintiq-pro-16.tablet

diff --git a/data/cintiq-pro-13.tablet b/data/cintiq-pro-13.tablet
new file mode 100644
index 0000000..197ad3f
--- /dev/null
+++ b/data/cintiq-pro-13.tablet
@@ -0,0 +1,45 @@
+# Wacom
+# Cintiq Pro 13
+# DTH-1320K0
+#
+#                       K K K K K
+#          *-----------------------*
+#          |                       |
+#          |                       |
+#          |                       |
+#          |                       |
+#          |                       |
+#          |        DISPLAY        |
+#          |                       |
+#          |                       |
+#          |                       |
+#          |                       |
+#          |                       |
+#          *-----------------------*
+#
+# Note: The device has 5 keys as shown above. Their
+#       intended uses are, from left to right,:
+#       1. Mode change (Display/Opaque)
+#       2. Wacom Desktop Center
+#       3. On screen keyboard
+#       4. Wacom display settings
+#       5. Touch on/off
+#
+
+[Device]
+Name=Wacom Cintiq Pro 13
+Class=Cintiq
+DeviceMatch=usb:056a:034F
+PairedID=usb:056a:0353
+Width=14
+Height=9
+# No pad buttons, so no layout
+Styli=0x842;0x84a;0x160802;0x16080a;0x100802;0x10080a;0x140802;0x14080a;0x120802;0x100804;0x10080c;0x100902;0x10090a
+IntegratedIn=Display
+
+[Features]
+Stylus=true
+Reversible=false
+Touch=true
+Ring=false
+Buttons=0
diff --git a/data/cintiq-pro-16.tablet b/data/cintiq-pro-16.tablet
new file mode 100644
index 0000000..e64bdd3
--- /dev/null
+++ b/data/cintiq-pro-16.tablet
@@ -0,0 +1,45 @@
+# Wacom
+# Cintiq Pro 16
+# DTH-1620K0
+#
+#                       K K K K K
+#          *-----------------------*
+#          |                       |
+#          |                       |
+#          |                       |
+#          |                       |
+#          |                       |
+#          |        DISPLAY        |
+#          |                       |
+#          |                       |
+#          |                       |
+#          |                       |
+#          |                       |
+#          *-----------------------*
+#
+# Note: The device has 5 keys as shown above. Their
+#       intended uses are, from left to right,:
+#       1. Mode change (Display/Opaque)
+#       2. Wacom Desktop Center
+#       3. On screen keyboard
+#       4. Wacom display settings
+#       5. Touch on/off
+#
+
+[Device]
+Name=Wacom Cintiq Pro 16
+Class=Cintiq
+DeviceMatch=usb:056a:0350
+PairedID=usb:056a:0354
+Width=16
+Height=10
+# No pad buttons, so no layout
+Styli=0x842;0x84a;0x160802;0x16080a;0x100802;0x10080a;0x140802;0x14080a;0x120802;0x100804;0x10080c;0x100902;0x10090a
+IntegratedIn=Display
+
+[Features]
+Stylus=true
+Reversible=false
+Touch=true
+Ring=false
+Buttons=0
-- 
2.9.3

